{"text_format":"1","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":223,"n_cols":9,"rows_kept":223,"cut":false,"hidden":false,"merged":[[3,3,3,5],[3,6,3,8],[0,0,2,8],[222,0,225,8]],"flags":["formulas_cached_only"]}
["Таблица совместимости принтеров с\nOPTION LAN PRINT"]
[]
[]
[null,null,null,"Windows XP/2003 Server",null,null,"Windows 7/2008 Server"]
["№","Производитель","Модель","Print","Scan","Reader","Print","Scan","Reader"]
[1,"Avision","MF3230","+","+*","Н/Ф","+","+*","Н/Ф"]
[2,"BenQ","CM3000","+","+","Н/Ф","+","+","Н/Ф"]
[3,"BenQ","CM3500","+","+","+","+","+","+"]
[4,"Brother","HL 2040","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[5,"Brother","HL 5250DN","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[6,"Brother","MFC-240C","+","+","+","+","+*","+"]
[7,"Brother","MFC-3820cn","+","+","-","+","+","-"]
[8,"Brother","MFC-3320cn","+","Н/Ф","-","-","Н/Ф","-"]
[9,"Brother","MFC-7420","+","+","Н/Ф","+","+*","Н/Ф"]
[10,"Canon","CanonScan Lide 5.0","Н/Ф","+","Н/Ф","Н/Ф","+","Н/Ф"]
[11,"Canon","ImageClass MF3110","+","+","Н/Ф","+","+","Н/Ф"]
[12,"Canon","ImageClass MF3112","-","-","-","-","-","-"]
[13,"Canon","ImageClass MF3220","-","-","-","-","-","-"]
[14,"Canon","ImageClass MF3222","-","-","-","-","-","-"]
[15,"Canon","ImageClass MF4010","+","+","Н/Ф","+","+","Н/Ф"]
[16,"Canon","ImageClass MF4150","+","+","Н/Ф","+","+","Н/Ф"]
[17,"Canon","iP100","-","-","-","-","-","-"]
[18,"Canon","iP1700 +",null,"Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[19,"Canon","iP2500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[20,"Canon","iP2600","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[21,"Canon","iP3300","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[22,"Canon","iP3500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[23,"Canon","iP3600","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[24,"Canon","iP4200","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[25,"Canon","iP4300","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[26,"Canon","iP4500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[27,"Canon","iP4600","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[28,"Canon","iP5000","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[29,"Canon","iP6700D","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[30,"Canon","iP7500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[31,"Canon","iP90","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[32,"Canon","iP90v","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[33,"Canon","iX5000","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[34,"Canon","LBP 1100","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[35,"Canon","LBP 3200","Н/Ф","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[36,"Canon","LBP 3300","Н/Ф","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[37,"Canon","LBP 3700","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[38,"Canon","MP110","-","-","-","-","-","-"]
[39,"Canon","MP130","+","+","+","+","+","+"]
[40,"Canon","MP145","-","-","-","-","-","-"]
[41,"Canon","MP150","+","+","Н/Ф","-","-","Н/Ф"]
[42,"Canon","MP160","-","-","-","-","-","-"]
[43,"Canon","MP170","-","-","-","-","-","-"]
[44,"Canon","MP180","-","-","-","-","-","-"]
[45,"Canon","MP450","+","+","+","+","+","+"]
[46,"Canon","MP460","+","+","+","+","+","+"]
[47,"Canon","MP470","+","+","+","+","+","+"]
[48,"Canon","MP480","+","+","+","-","+","+"]
[49,"Canon","MP510","+","+","+","+","+","+"]
[50,"Canon","MP520","+","+","+","+","+","+"]
[51,"Canon","MP540","+","+","+","-","+","+"]
[52,"Canon","MP600","+","+","+","+","+","+"]
[53,"Canon","MP610","+","+","+","+","+","+"]
[54,"Canon","MP620","+","+","+","-","+","+"]
[55,"Canon","MP630","+","+","+","-","+","+"]
[56,"Canon","MP730","+","+","Н/Ф","+","+","Н/Ф"]
[57,"Canon","MP780","+","+","Н/Ф","+","+","Н/Ф"]
[58,"Canon","MP810","+","+","-","+","-","-"]
[59,"Canon","MP830","+","+","+","+","+","+"]
[60,"Canon","MP960","+","+","+","+","+","+"]
[61,"Canon","MP970","+","+","+","+","+","+"]
[62,"Canon","MP980","+","+","+","-","+","+"]
[63,"Canon","MX308","+","+","Н/Ф","+","+","Н/Ф"]
[64,"Canon","MX700","-","-","-","+","-","-"]
[65,"Canon","MX7600 +",null,"+","+","+","+","+"]
[66,"Canon","MX850","+","+","+","+","+","+"]
[67,"Canon","Pixus 990i","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[68,"Canon","Pro9000","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[69,"Canon","Pro9000 Mark II","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[70,"Canon","Pro9500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[71,"Canon","Pro9500 Mark II","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[72,"Dell","Photo 720","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[73,"Epson","AL-C900","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[74,"Epson","EPL-5800","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[75,"Epson","EPL-6200L","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[76,"Epson","EPL-N2500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[77,"Epson","LP 2500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[78,"Epson","Perfection 1270","Н/Ф","+","Н/Ф","-","+","Н/Ф"]
[79,"Epson","PM-100","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[80,"Epson","PM-3700C","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[81,"Epson","PM-A840","+","+","+","+","+","+"]
[82,"Epson","PM-A840S","-","-","-","+","-","-"]
[83,"Epson","PM-A950","+","Н/Ф","+","+","Н/Ф","+"]
[84,"Epson","PM-G4500","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[85,"Epson","PM-G5300","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[86,"Epson","PM-G860","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[87,"Epson","PM-T940","+","+","+","+","+","+"]
[88,"Epson","PM-T960","+","+","+","+","+","+"]
[89,"Epson","PM-T990","+","+","+","+","+","+"]
[90,"Epson","PX-501A","-","-","-","+","-","-"]
[91,"Epson","PX-5600","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[92,"Epson","PX-5800","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[93,"Epson","PX-A640","+","+","+","+","+","+"]
[94,"Epson","PX-A740","+","+","+","+","+","+"]
[95,"Epson","PX-FA700","+","+","+","+","+","+"]
[96,"Epson","PX-V780","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[97,"Epson","Stylus C43UX","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[98,"Epson","Stylus C45","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[99,"Epson","Stylus C60","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[100,"Epson","Stylus C61","-","-","-","-","-","-"]
[101,"Epson","Stylus C65","-","-","-","-","-","-"]
[102,"Epson","Stylus C66","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[103,"Epson","Stylus C67","-","-","-","-","-","-"]
[104,"Epson","Stylus C90","-","-","-","-","-","-"]
[105,"Epson","Stylus Color 670","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[106,"Epson","Stylus CX2900","+","+","Н/Ф","+","+","Н/Ф"]
[107,"Epson","Stylus CX3500","+","+","Н/Ф","+","+","Н/Ф"]
[108,"Epson","Stylus CX3700","-","-","-","-","-","-"]
[109,"Epson","Stylus CX3810","+","+","Н/Ф","-","-","Н/Ф"]
[110,"Epson","Stylus CX3900","+","+","Н/Ф","+","+","Н/Ф"]
[111,"Epson","Stylus CX4700","+","+","Н/Ф","+","+","Н/Ф"]
[112,"Epson","Stylus CX4800","+","-","-","-","-","-"]
[113,"Epson","Stylus CX4900","+","+","-","+","+","-"]
[114,"Epson","Stylus CX9300F","+","+","+","+","+","+"]
[115,"Epson","Stylus Photo 1270","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[116,"Epson","Stylus Photo 2200","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[117,"Epson","Stylus Photo 830","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[118,"Epson","Stylus Photo 915","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[119,"Epson","Stylus R310","+","Н/Ф","+","+","Н/Ф","+"]
[120,"Epson","Stylus R320","+","Н/Ф","+","-","Н/Ф","+"]
[121,"Epson","Stylus RX510","+","+","+","+","+","+"]
[122,"Epson","Stylus RX530","+","+","+","+","+","+"]
[123,"Epson","Stylus RX590","+","+","+","-","-","-"]
[124,"Hewlett-Packard ","Deskjet 1125C","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[125,"Hewlett-Packard ","Deskjet 1180C","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[126,"Hewlett-Packard ","Deskjet 1220C","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[127,"Hewlett-Packard ","Deskjet 3745","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[128,"Hewlett-Packard ","Deskjet 5652","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[129,"Hewlett-Packard "," Deskjet 640C","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[130,"Hewlett-Packard "," Deskjet 830C","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[131,"Hewlett-Packard ","Deskjet 920C","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[132,"Hewlett-Packard "," Deskjet D2360","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[133,"Hewlett-Packard ","Deskjet D2460","-","-","-","-","-","-"]
[134,"Hewlett-Packard ","Deskjet D3745","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[135,"Hewlett-Packard ","Deskjet D4160","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[136,"Hewlett-Packard ","Deskjet D4260","-","-","-","-","-","-"]
[137,"Hewlett-Packard "," Deskjet F300","+","+","Н/Ф","+","+","Н/Ф"]
[138,"Hewlett-Packard ","Deskjet F340","-","-","-","-","-","-"]
[139,"Hewlett-Packard "," Deskjet F350","-","-","-","-","-","-"]
[140,"Hewlett-Packard ","Deskjet F370","-","-","+","-","-","+"]
[141,"Hewlett-Packard ","Deskjet F379","-","-","+","-","-","+"]
[142,"Hewlett-Packard ","Deskjet F380","-","-","+","-","-","+"]
[143,"Hewlett-Packard ","Deskjet F4185","+","+","Н/Ф","+","+","Н/Ф"]
[144,"Hewlett-Packard "," LaserJet 1000","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[145,"Hewlett-Packard ","LaserJet 1010","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[146,"Hewlett-Packard ","LaserJet 1015","-","-","-","+","-","-"]
[147,"Hewlett-Packard "," LaserJet 1018","+","Н/Ф","Н/Ф","NS","Н/Ф","Н/Ф"]
[148,"Hewlett-Packard "," LaserJet 1020","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[149,"Hewlett-Packard "," LaserJet 1022","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[150,"Hewlett-Packard ","LaserJet 1160","+","Н/Ф","Н/Ф","NS","Н/Ф","Н/Ф"]
[151,"Hewlett-Packard "," LaserJet 2420","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[152,"Hewlett-Packard ","LaserJet 2600n","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[153,"Hewlett-Packard ","LaserJet 3015","+","+","Н/Ф","-","+","Н/Ф"]
[154,"Hewlett-Packard "," LaserJet 3030","+","-","-","+","-","-"]
[155,"Hewlett-Packard "," LaserJet 3050","+","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф"]
[156,"Hewlett-Packard "," LaserJet 3050z","-","-","-","+","-","-"]
[157,"Hewlett-Packard ","LaserJet 3330","+","+","Н/Ф","+","+","Н/Ф"]
[158,"Hewlett-Packard ","LaserJet 3380","-","-","-","+","-","-"]
[159,"Hewlett-Packard ","LaserJet M1005","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[160,"Hewlett-Packard ","Officejet 4255","+","+","Н/Ф","+","+","Н/Ф"]
[161,"Hewlett-Packard ","Officejet 5510","+","+","Н/Ф","+","+","Н/Ф"]
[162,"Hewlett-Packard "," Officejet 5610","+","+","Н/Ф","+","+","Н/Ф"]
[163,"Hewlett-Packard ","Officejet 6210","+","+","Н/Ф","-","+","Н/Ф"]
[164,"Hewlett-Packard ","Officejet 7210","+","+","+","+","+","+"]
[165,"Hewlett-Packard ","Officejet G85","+","+","Н/Ф","-","+","Н/Ф"]
[166,"Hewlett-Packard ","Officejet Pro L7380","+","+","Н/Ф","+","+","Н/Ф"]
[167,"Hewlett-Packard ","PhotoSmart 2610","+","+","+","+","+","+"]
[168,"Hewlett-Packard ","PhotoSmart 3110","+","+","+","+","+","+"]
[169,"Hewlett-Packard ","PhotoSmart 3210","+","+","+","+","+","+"]
[170,"Hewlett-Packard "," PhotoSmart 3310","-","-","-","+","-","-"]
[171,"Hewlett-Packard "," PhotoSmart 335","+","+","+","+","+","+"]
[172,"Hewlett-Packard ","PhotoSmart 7830","+","Н/Ф","+","+","Н/Ф","+"]
[173,"Hewlett-Packard ","PhotoSmart 8030","+","+","+","+","+","+"]
[174,"Hewlett-Packard ","PhotoSmart A310","+","Н/Ф","Н/Ф","-","Н/Ф","Н/Ф"]
[175,"Hewlett-Packard "," PhotoSmart C3180","+","+","+","+","+","+"]
[176,"Hewlett-Packard ","PhotoSmart C5280","+","+","+","+","+","+"]
[177,"Hewlett-Packard ","PhotoSmart P1000","+","Н/Ф","+","-","Н/Ф","+"]
[178,"Hewlett-Packard ","PSC 1210","+","+","Н/Ф","+","+","Н/Ф"]
[179,"Hewlett-Packard ","PSC 1315","+","+","Н/Ф","+","+","Н/Ф"]
[180,"Hewlett-Packard ","PSC 1350","+","+","+","+","+","+"]
[181,"Hewlett-Packard ","PSC 1402","-","-","-","+","-","-"]
[182,"Hewlett-Packard ","PSC 1410","+","+","Н/Ф","+","+","Н/Ф"]
[183,"Hewlett-Packard ","PSC 1510","-","-","-","+","-","-"]
[184,"Hewlett-Packard ","PSC 1610","+","+","+","+","+","+"]
[185,"Hewlett-Packard ","PSC 2210 All-in-one","+","+","-","-","+","-"]
[186,"Hewlett-Packard ","PSC 2410 All-in-one","-","-","-","+","-","-"]
[187,"Hewlett-Packard ","PSC 2510 All-in-one","+","+","+","-","+","+"]
[188,"Hewlett-Packard ","Scanjet 4200C","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф","+*"]
[189,"Hewlett-Packard ","Scanjet 4370","Н/Ф","Н/Ф","+","Н/Ф","Н/Ф","+"]
[190," Konica Minota","MC-2430DL","+","+","Н/Ф","Н/Ф","-","Н/Ф"]
[191," Konica Minota","Page Pro 1350W","Н/Ф","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[192,"Lexmark","E120","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[193,"Lexmark","P4350","+","+","+","+","+","+"]
[194,"Lexmark","P6250","+","+","+","+","+","+"]
[195,"Lexmark","X1270","+","+","+*","Н/Ф","+","+*"]
[196,"Lexmark","X2250","+","+","+","Н/Ф","+","+"]
[197,"Lexmark","X2650","+","+","+","-","+","+"]
[198,"Lexmark","X3350","+","+","+","Н/Ф","+","+"]
[199,"Lexmark","X3470","+","+","+*","+","+","+*"]
[200,"Lexmark","X3550","+","+","+*","+","+","+*"]
[201,"Lexmark","X4270","+","+","+","-","+","+"]
[202,"Lexmark","X5150","+","+","+","Н/Ф","+","+*"]
[203,"Lexmark","X5470","+","+","+","+","+","+"]
[204,"Lexmark","X5495","+","+","+","-","+","+"]
[205,"Lexmark","X6170","+","+","+","Н/Ф","+","+"]
[206,"Lexmark","X7350","+","+","+*","Н/Ф","+","+*"]
[207,"Lexmark","X8350","+","+","+","Н/Ф","+","+"]
[208,"Lexmark","Z1350","+","+","-","-","+","-"]
[209,"Lexmark","Z43","Н/Ф","+","Н/Ф","Н/Ф","Н/Ф","Н/Ф"]
[210,"Lexmark","Z55","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[211,"Lexmark","Z705","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[212,"OKI","B4350","+","Н/Ф","Н/Ф","Н/Ф","+","Н/Ф"]
[213,"Samsung","ML-1710","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[214,"Samsung","ML-1750","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[215,"Samsung","ML-2010","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[216,"Samsung","SCX 4016","+","+","Н/Ф","Н/Ф","+","Н/Ф"]
[217,"Samsung","SCX 4500","+","+","+","Н/Ф","+","+"]
["+         прошел тестирование\n*       требует установки програмного обеспечения для реализации функций\n-          не подходит для данной операционной системы\nН/Ф   этой функции нет в данной модели"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}